For selecting any new RVP, there is a constraint that it has to be achieved:

The newly added sensors by the new RVP has to be more than PR=total number of sensors /number of RVP

Number of sensors in the environment is 100

Number of RV points is 10

🡪 in average each RV point has to add to the coverage 100/10=10 new nodes